SOFT X-RAY APERTURE

ANODES

STEEL COVER

Fe^{55}

OPENING IN THE INSTRUMENT COVER

APERTURE DETAILS

1.2mm

GLASS SEALING

mm mm

5

mm

W.N W.N

1.85

12.5

3.8

BE 150 FILTER um

BE 150 FILTER um